NEWSLETTER

New RAILBEAM model TN 406 W

Bogie pressure up to 2500KN

The new standards are asking for bigger partial coefficients.

We therefore have designed a new RAILBEAM, TN406 W ,

The New welded design were tested February 2016 together with

Tallinn University Estonia. The welding of a UIC 60 RAIL were done by

preheating the rail and welded by a mangan wire.

The TN406W is based on the idea that the rail and beam is welded together

and hereby giving a 66 % bigger moment of inertia.

The new mono profile unit is giving a load capacity of 2500kN (250 TON)

For further information contact Erik Lohmann or John Sander

Please see www.railbeam.com